GySEV Árpád gyorssínautóbusz, v1.0

A virtuális modellt készítette: George33 (george33@vipmail.hu), 2006.
A textúrák saját fotók alapján készültek.

Installálás:
	Először csomagold ki az Arpad.zip könyvtárat a ..\Trains\Trainset mappába.
	Készíts egy Consistot, és indulhatsz!

A modell problémái és hiányosságai:
	1. A vezetőfülke egyelőre ideiglenes. Közeljövőben várhatóan készül egy jobb.
	2. A sebességváltókar működése eltés az eredetitől, mivel a közbenső üres fokozatokban visszaugrik
	    "0" pozícióba. Eredeti állások: 0>Indít>1>0>2>0>3>0>4>5.
	3. A sebességváltó áttételei nem eredetiek. A menetszabályzó (gáz) működése nem realisztikus.
	4. A fékkar nem ugrik vissza alaphelyzetbe, mint az eredetiben.

A modell Freeware, szabadon terjeszthető.
3D modell: gmax (www.autodesk.com)
Köszönet a tesztelésért
Jó vonatozást!

http://george33.fw.hu/
www.freewebs.com/george33
--------------------------------------------------------------------------------------------------------------

Historic Ganz Railcar, "Arpad", made in 1934, v1.0

Technical Data:
	Locomotive type: Diesel-mechanical, 5 gears.
	Power source: originally a 163 kW Ganz-Jendrassik Diesel engine.
	Max. speed: 120 km/h (76 mph).
	Wheel configuration: Eight wheels in B-2 configuration.

Virtual model and fotos by George33 (george33@vipmail.hu), 2006.

Installation:
	First unzip the Arpad.zip into the..\Trains\Trainset folder.
	Make a Consist and go!

Help for driving the railcar:
	Basically the brakes are released (central position).
	Drop the reverser to "forward" position (W).
	Start moving: switch the gear lever to the first position (E).
	Then increase the throttle: 20-40-60-80-100 (D).
	If you reached the speed 25 km/h, decrease the trottle to the position 60 or 40 (A).
	Switch the gear ->0->2 (E,E).
	You can accelerate by increasing throttle.
	Peak values of speed in each gears: 28, 40, 60, 83, 120 km/h.
	To stop the train decrease the trottle to 0 (A).
	Switch the gear to the next "0" position (Shift+E).
	Push brake lever a moment to the right, then back (';).
	Aftter that you can hear the noise of brake-shoes.
	You can increase the brake force in short periodes to make a stop.
	In case of  too strong deceleration you can release brakes by pushing the lever to the left (;').
	After stopping switch the gear to basic position (Shift+E), after that release brakes!
	Caution! In reverse position it's an error in the Train Simulator program!

Known problems and defects:
	1. The forward cabview is a temporary solution, there will be a better soon.
	2. Operation of the gear lever doesn't equal to the original, in the "none" positions jumps back to the basic.
	    Original positions: 0>Start>1>0>2>0>3>0>4>5.
	3. The gear transmissions are not equal to the original. Operation of the throttle isn't realistic.
	4. The brake lever doesn't jump back to the basic position, as it does in the original railcar.

This model is freeware.
3D model created using gmax (www.autodesk.com)
Thanks to my friend ... for testing this model.
Have fun!

http://george33.fw.hu/
www.freewebs.com/george33